# Abstract

We landed on the Moon a little less than fifty years ago, and human beings will potentially colonize a second planet in near future. The most possible option is Mars. NASA and some private organizations are presently planning to send human missions to Mars within 2030s. Rather than just setting down a simple footprint, however, this will be a more advanced step: the establishment of a successful and durable habitat on the Martian surface. Humankind has an enduring history of survival and adaptation. Considering the advancements made via science and engineering technology, experts already believe that survival on a distant planet is possible – even within a hostile environment such as Mars. Yet, survival is not enough to declare a habitat as successful one. Especially on Mars, it is difficult to ensure a healthy environment for both physiological and psychological conditions within a confined habitat. Perhaps, the most arduous challenge will be to create (or recreate) the feeling of a

„Home‟ where our human crews will not just survive but will in fact thrive!

This report explores an overall portrayal of the extreme environmental conditions of Mars and the obstacles to be faced by those first human crews. Finally, through the case studies and their cross analysis, this research will reveal the plausible solutions for the most challenging problem regarding the first Martian habitat: How architecture can construct a viable and sustainable shelter for an extremely hostile environment and simultaneously, establish a new identity for the „Universal Home‟ on another planet.

**Key words:** Mars habitation, Extreme environment, Construction on Mars, Universal home.

# Introduction

*“He who will one day teach men to fly will have moved all boundary-stones; all boundary-stones will themselves fly into the air to him, he will baptize the earth anew – as the weightless”*

Friedrich Nietzsche, Thus Spoke Zarathustra

(1883 – 1885) [1]

I do not think Friedrich Nietzsche thought about inter planetary flying here, however, his words “moved all boundary-stones” reflects human beings present and future curious and passionate steps to the world of unknown. Designing for Outer Space (above the atmosphere) is not the thing architects usually do. At present, we know how to survive in space (near Earth‟s orbit) and the next step will be how to live on a neighbor planet. Between the two nearest possible options – Mars and Venus, Mars is more suitable for human colonization. The focus of this paper concerns „MARS Habitation – in an extreme environmental condition‟. Therefore, questions arise concerning the category of the habitation on Mars: will it be a temporary or a permanent solution, what types of extreme environment do we need to consider for protection, how should we approach design for this protection, what are the most suitable building materials and what will be the construction process? Finally, what will be the psychological effects on those inhabitants? Overall, what can architecture do to solve these problems? In this paper, I will try to find the answers of these questions trough two hypothetical case studies (“The Ice House” by Clouds Architecture and “The Modular Habitat” by Foster and Partners) along with two existing examples of International Space Station and a research station in Antarctica.

# Mission Mars

Since the 20th century, there have been several proposed human missions to Mars both by government agencies and private companies.

Most of the human mission concepts as currently conceived by national governmental space programs would not be direct precursors to colonization. Programs such as those being tentatively planned by NASA, Roscosmos, and ESA are intended solely as exploration missions, with the establishment of a permanent base possible but not yet the main goal.

Colonization requires the establishment of permanent habitats that have the potential for self-expansion and self-sustenance. Two early proposals for building habitats on Mars are the Mars Direct and the Semi-Direct concepts, advocated by Robert Zubrin, an advocate of the colonization of Mars.[1]

At the February 2017 World Government Summit, the United Arab Emirates announced a plan to establish a settlement on Mars by 2117, led by the Mohammed bin Rashid Space Centre.[2][3]

SpaceX has proposed the development of Mars transportation infrastructure in order to facilitate the eventual colonization of Mars. The mission architecture includes fully reusable launch vehicles, human-rated spacecraft, on-orbit propellant tankers, rapid-turnaround launch/landing mounts, and local production of rocket fuel on Mars via in situ resource utilization (ISRU). SpaceX's aspirational goal as of 2017 was to land their cargo Starships on Mars by 2024 and the first 2 crewed starships by 2026.[4][5]

# Who will go to Mars?

To design the first habitat on Mars, the main consideration will be – who will use it? In other words, who will go to Mars? Both NASA and some other private organizations (like, Space-X and Mars One) are planning to send Manned mission to Mars and their target year is around 2030. However, there is a basic difference in their strategies. NASA is planning to send a small group of astronauts cum scientists, who will land on Mars, stay for a while and come back. On the other hand, these private organizations are planning to send some selected and trained common people to stay there forever. Eventually the habitat design for these two groups will be quite different from each other. Personally, I believe, we need to wait to send a one way manned mission to Mars until a successful return mission is completed as planned by NASA. Therefore, in this

paper, I will discuss about the habitat, which will be suitable for staying on Mars for a limited period of time and after that can be reused as a base for the next permanent habitat.

However, no matter which group will go to the Mars first, each person of every group will be well trained and tested for several times both physically and mentally. As Physician Jerri Nielson (a legend of ultimate survival in a life and death situation in Antarctica) in her account of living at the Amundsen-Scott South Pole Station writes*, “living in extreme conditions requires a flexible intelligence, where the ability to quickly absorb and react to new situations is a valuable asset. They wanted to weed out people with personality disorders, chronic complainers, the chronically depressed, substance abusers…”* [2] [Nielsen with Vollers, Ice bound] Yet, we are able to lessen the extremities of physical and psychological sufferings through our concerned architectural solutions, as the following discussion suggest a means to do so.

# Methodology:

A comparative case study analysis of “The Ice House” by Clouds architecture and “the Modular Habitat” by Foster and partners is conducted to find suitable answers to hypothetical and existing built environments with approximately similar conditions: near orbital space stations and polar area shelter in extreme climatic zone. In addition, through a discussion of the technical (alien climate, hostile nature inclusive of radiation

and gravity, construction materials and process) and non-technical issues (living indoor with low atmospheric pressure, psychological effects, and design form and concept) and a cross analysis of these case studies, I hope to arrive at a better understanding of the challenges of mars habitation. Finally, I shall propose the plausible design strategies for designing a habitat in Mars.

# Comparisons between Earth and Mars

## Gravity and size[[edit](https://en.wikipedia.org/w/index.php?title=Colonization_of_Mars&action=edit&section=3)]

The surface [gravity of Mars](https://en.wikipedia.org/wiki/Gravity_of_Mars) is just 38% that of Earth. Although [microgravity](https://en.wikipedia.org/wiki/Microgravity) is known to cause health problems such as [muscle loss and bone demineralization](https://en.wikipedia.org/wiki/Weightlessness#Human_health_effects),[[7]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-WIRED-20140212-7)[[8]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-8) it is not known if Martian gravity would have a similar effect. The [Mars Gravity Biosatellite](https://en.wikipedia.org/wiki/Mars_Gravity_Biosatellite) was a proposed project designed to learn more about what effect Mars' lower surface gravity would have on humans, but it was cancelled due to a lack of funding.[[9]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-9)

Mars has a surface area that is 28.4% of Earth's, which is only slightly less than the amount of dry land on Earth (which is 29.2% of Earth's surface). Mars has half the radius of Earth and only one-tenth the mass. This means that it has a smaller volume (≈15%) and lower average density than Earth.

## Magnetosphere[[edit](https://en.wikipedia.org/w/index.php?title=Colonization_of_Mars&action=edit&section=4)]

Due to the lack of a [magnetosphere](https://en.wikipedia.org/wiki/Magnetosphere), [solar particle events](https://en.wikipedia.org/wiki/Solar_particle_event) and [cosmic rays](https://en.wikipedia.org/wiki/Cosmic_ray) can easily reach the Martian surface.[[10]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-solar_wind_at_Mars-10)[[11]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-hostile_to_life-11)[[12]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-12)

## The atmosphere[[edit](https://en.wikipedia.org/w/index.php?title=Colonization_of_Mars&action=edit&section=5)]

[Atmospheric pressure](https://en.wikipedia.org/wiki/Atmospheric_pressure) on Mars is far below the [Armstrong limit](https://en.wikipedia.org/wiki/Armstrong_limit) at which people can survive without [pressure suits](https://en.wikipedia.org/wiki/Pressure_suit). Since [terraforming](https://en.wikipedia.org/wiki/Terraforming_of_Mars) cannot be expected as a near-term solution, habitable structures on Mars would need to be constructed with [pressure vessels](https://en.wikipedia.org/wiki/Pressure_vessel) similar to spacecraft, capable of containing a pressure between 30 and 100 kPa. The atmosphere is also toxic as most of it consists of [carbon dioxide](https://en.wikipedia.org/wiki/Carbon_dioxide) (95% [carbon dioxide](https://en.wikipedia.org/wiki/Carbon_dioxide), 3% nitrogen, 1.6% argon, and traces totaling less than 0.4% of other gases, including oxygen).

This thin atmosphere does not filter out [ultraviolet sunlight](https://en.wikipedia.org/wiki/Health_effects_of_sunlight_exposure), which causes instability in the molecular bonds between atoms. For example, ammonia (NH3) is not stable in the Martian atmosphere and breaks down after a few hours.[[13]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-davidw-13) Also due to the thinness of the atmosphere, the temperature difference between day and night is much larger than on Earth, typically around 70 °C (125 °F).[[14]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-REMS-2015-14) However, the day/night temperature variation is much lower during dust storms when very little light gets through to the surface even during the day, and instead warms the middle atmosphere.[[15]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-Opportunity_Hunkers_Down_During_Dust_Storm-15)

## Water and climate[[edit](https://en.wikipedia.org/w/index.php?title=Colonization_of_Mars&action=edit&section=6)]

[Water on Mars](https://en.wikipedia.org/wiki/Water_on_Mars) is scarce, with rovers [*Spirit*](https://en.wikipedia.org/wiki/Spirit_(rover)) and [*Opportunity*](https://en.wikipedia.org/wiki/Opportunity_(rover)) finding less than there is in Earth's driest desert.[[16]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-Why_is_Mars_So_Dry-16)[[17]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-17)[[18]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-NASA-20131210-18)

The [climate](https://en.wikipedia.org/wiki/Climate_of_Mars) is much colder than Earth, with mean surface temperatures between 186 and 268 K (−87 and −5 °C; −125 and 23 °F) (depending on the season and latitude).[[19]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-19)[[20]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-20) The [lowest temperature ever recorded on Earth](https://en.wikipedia.org/wiki/Extremes_on_Earth) was 184 K (−89.2 °C, −128.6 °F) in [Antarctica](https://en.wikipedia.org/wiki/Antarctica).

Because Mars is about 52% farther from the [Sun](https://en.wikipedia.org/wiki/Sun), the amount of [solar energy](https://en.wikipedia.org/wiki/Solar_energy) entering its upper atmosphere per unit area (the [solar constant](https://en.wikipedia.org/wiki/Solar_constant)) is only around 43.3% of what reaches the Earth's upper atmosphere.[[21]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-21) However, due to the much thinner atmosphere, a higher fraction of the solar energy reaches the surface as radiation.[[22]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-22)[[23]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-23) The maximum solar irradiance on Mars is about 590 W/m2 compared to about 1000 W/m2 at the Earth's surface; optimal conditions on the Martian equator can be compared to those on [Devon Island](https://en.wikipedia.org/wiki/Devon_Island) in the Canadian Arctic in June.[[24]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-tomatoes-24) Mars' orbit is more [eccentric](https://en.wikipedia.org/wiki/Eccentricity_(orbit)) than Earth's, increasing temperature and solar constant variations over the course of the Martian year.[[*citation needed*](https://en.wikipedia.org/wiki/Wikipedia:Citation_needed)] Mars has no rain and virtually no clouds,[[*citation needed*](https://en.wikipedia.org/wiki/Wikipedia:Citation_needed)] so although cold, it is permanently sunny (apart from during [dust storms](https://en.wikipedia.org/wiki/Climate_of_Mars#Dust_storms)). This means solar panels can always operate at maximum efficiency on dust-free days.

[Global dust storms](https://en.wikipedia.org/wiki/Climate_of_Mars#Effect_of_dust_storms) are common throughout the year and can cover the entire planet for weeks, blocking sunlight from reaching the surface.[[25]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-25)[[26]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-26) This has been observed to cause temperature drops of 4 °C (7 °F) for several months after the storm.[[27]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-Fenton-27) In contrast, the only comparable events on Earth are infrequent large volcanic eruptions such as the [Krakatoa](https://en.wikipedia.org/wiki/Krakatoa) event which threw large amounts of ash into the atmosphere in 1883, causing a global temperature drop of around 1 °C (2 °F). These dust storms would affect electricity production from solar panels for long periods, and interfere with communications with Earth.[[15]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-Opportunity_Hunkers_Down_During_Dust_Storm-15)

## Temperature and seasons[[edit](https://en.wikipedia.org/w/index.php?title=Colonization_of_Mars&action=edit&section=7)]

Mars has an [axial tilt](https://en.wikipedia.org/wiki/Axial_tilt) of 25.19°, similar to Earth's 23.44°. As a result, Mars has [seasons](https://en.wikipedia.org/wiki/Season) much like Earth, though on average they last nearly twice as long because the Martian year is about 1.88 Earth years. Mars' temperature regime is more similar to Earth's than all other planets‘ in the solar system. While generally colder than Earth, Mars can have Earth-like temperatures in some areas and at certain times.

## Soil[[edit](https://en.wikipedia.org/w/index.php?title=Colonization_of_Mars&action=edit&section=8)]

The [Martian soil is toxic](https://en.wikipedia.org/wiki/Martian_soil#Toxicity) due to relatively high concentrations of chlorine and associated compounds, such as perchlorates, which are hazardous to all known forms of life.[[28]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-toxicsoil1-28)[[29]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-toxicmars-29)

## Survivability[[edit](https://en.wikipedia.org/w/index.php?title=Colonization_of_Mars&action=edit&section=9)]

Plants and animals cannot survive the ambient conditions on the surface of Mars.[[30]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-30) However, some [extremophile](https://en.wikipedia.org/wiki/Extremophile) organisms that survive in hostile conditions on Earth have endured periods of exposure to environments that approximate some of the conditions found on Mars.

## Length of day[[edit](https://en.wikipedia.org/w/index.php?title=Colonization_of_Mars&action=edit&section=10)]

The Martian day (or [sol](https://en.wikipedia.org/wiki/Sol_(day_on_Mars))) is very close in duration to Earth's. A [solar day](https://en.wikipedia.org/wiki/Solar_day) on Mars is 24 hours, 39 minutes and 35.244 seconds.[[31]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-31)

## Conditions for human habitation[[edit](https://en.wikipedia.org/w/index.php?title=Colonization_of_Mars&action=edit&section=11)]

[](https://en.wikipedia.org/wiki/File:Project_Deimos_-_Mars_Surface_Base.jpg)

An expedition-style crewed mission would operate on the surface, but for limited amounts of time

[](https://en.wikipedia.org/wiki/File:Mars-human-exploration-art-astronauts-vehicle-dust-full.jpg)

[Dust](https://en.wikipedia.org/wiki/Dust) is one concern for Mars missions

Conditions on the surface of Mars are closer to the conditions on Earth in terms of temperature and sunlight than on any other planet or moon, except for the [cloud tops of Venus](https://en.wikipedia.org/wiki/Colonization_of_Venus#Aerostat_habitats_and_floating_cities).[[32]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-32) However, the surface is not hospitable to humans or most known life forms due to the radiation, greatly reduced air pressure, and an atmosphere with only 0.16% oxygen.

In 2012, it was reported that some [lichen](https://en.wikipedia.org/wiki/Lichen) and [cyanobacteria](https://en.wikipedia.org/wiki/Cyanobacteria) survived and showed remarkable [adaptation capacity](https://en.wikipedia.org/wiki/Adaptive_capacity) for [photosynthesis](https://en.wikipedia.org/wiki/Photosynthesis) after 34 days in [simulated](https://en.wikipedia.org/wiki/Simulation) [Martian conditions](https://en.wikipedia.org/wiki/Life_on_Earth_under_Martian_conditions) in the Mars Simulation Laboratory (MSL) maintained by the [German Aerospace Center](https://en.wikipedia.org/wiki/German_Aerospace_Center) (DLR).[[33]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-Skymania-20120426-33)[[34]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-EGU-20120426-34)[[35]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-dlr-35) Some scientists think that cyanobacteria could play a role in the development of self-sustainable crewed outposts on Mars.[[36]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-Verseux2015-36) They propose that cyanobacteria could be used directly for various applications, including the production of food, fuel and oxygen, but also indirectly: products from their culture could support the growth of other organisms, opening the way to a wide range of life-support biological processes based on Martian resources.[[36]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-Verseux2015-36)

Humans have explored parts of Earth that match some conditions on Mars. Based on NASA rover data, temperatures on Mars (at low latitudes) are similar to those in [Antarctica](https://en.wikipedia.org/wiki/Antarctica).[[37]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-37) The atmospheric pressure at the highest altitudes reached by [piloted balloon](https://en.wikipedia.org/wiki/High_altitude_balloon) ascents (35 km (114,000 feet) in 1961,[[38]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-38) 38 km in 2012) is similar to that on the surface of Mars. However, the pilots were not exposed to the extremely low pressure, as it would have killed them, but seated in a pressurized capsule.[[39]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-39)

Human survival on Mars would require living in artificial [Mars habitats](https://en.wikipedia.org/wiki/Mars_habitat) with complex life-support systems. One key aspect of this would be water processing systems. Being made mainly of water, a human being would die in a matter of days without it. Even a 5–8% decrease in total body water causes fatigue and dizziness and a 10% decrease physical and mental impairment (See [Dehydration](https://en.wikipedia.org/wiki/Dehydration)). A person in the [UK](https://en.wikipedia.org/wiki/UK) uses 70–140 litres of water per day on average.[[40]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-average-water-usage-40) Through experience and training, astronauts on the ISS have shown it is possible to use far less, and that around 70% of what is used can be recycled using the [ISS water recovery systems](https://en.wikipedia.org/wiki/ISS_ECLSS#Water_recovery_systems). (For instance, half of all water is used during showers.[[41]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-41)) Similar systems would be needed on Mars but would need to be much more efficient, since regular robotic deliveries of water to Mars would be prohibitively expensive (the ISS is supplied with water four times per year). Potential access to on-site water (frozen or otherwise) via drilling has been investigated by NASA.[[42]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-42)

### Effects on human health**[**[**edit**](https://en.wikipedia.org/w/index.php?title=Colonization_of_Mars&action=edit&section=12)**]**

*Main article:*[*Effect of spaceflight on the human body*](https://en.wikipedia.org/wiki/Effect_of_spaceflight_on_the_human_body)

Mars presents a hostile environment for human habitation. Different technologies have been developed to assist long-term space exploration and may be adapted for habitation on Mars. The existing record for the longest consecutive space flight is 438 days by cosmonaut [Valeri Polyakov](https://en.wikipedia.org/wiki/Valeri_Polyakov" \o "Valeri Polyakov),[[43]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-nytimes-43) and the most accrued time in space is 878 days by [Gennady Padalka](https://en.wikipedia.org/wiki/Gennady_Padalka).[[44]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-Record_Breaking-44) The longest time spent outside the protection of the Earth's [Van Allen radiation belt](https://en.wikipedia.org/wiki/Van_Allen_radiation_belt) is about 12 days for the [Apollo 17](https://en.wikipedia.org/wiki/Apollo_17) moon landing. This is minor in comparison to the 1100-day journey to Mars and back[[45]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-45) envisioned by NASA for possibly as early as the year 2028. Scientists have also hypothesized that many different biological functions can be negatively affected by the environment of Mars colonies. Due to higher levels of radiation, there are a multitude of physical side-effects that must be mitigated.[[46]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-46) In addition, [Martian soil](https://en.wikipedia.org/wiki/Martian_soil#Toxicity) contains high levels of toxins which are hazardous to human health.

#### Physical effects**[**[**edit**](https://en.wikipedia.org/w/index.php?title=Colonization_of_Mars&action=edit&section=13)**]**


The difference in gravity may negatively affect human health by weakening [bones](https://en.wikipedia.org/wiki/Bone) and [muscles](https://en.wikipedia.org/wiki/Muscle). There is also risk of [osteoporosis](https://en.wikipedia.org/wiki/Osteoporosis) and [cardiovascular](https://en.wikipedia.org/wiki/Circulatory_system) problems. Current rotations on the [International Space Station](https://en.wikipedia.org/wiki/International_Space_Station) put astronauts in zero gravity for six months, a comparable length of time to a one-way trip to Mars. This gives researchers the ability to better understand the physical state that astronauts going to Mars would arrive in. Once on Mars, surface gravity is only 38% of that on Earth. Microgravity affects the cardiovascular, musculoskeletal and neurovestibular (central nervous) systems. The cardiovascular effects are complex. On Earth, blood within the body stays 70% below the heart, but in microgravity this is the not case due to nothing pulling the blood down. This can have several negative effects. Once entering into microgravity, the blood pressure in the lower body and legs is significantly reduced.[[47]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-47) This causes legs to become weak through loss of muscle and bone mass. Astronauts show signs of a puffy face and chicken legs syndrome. After the first day of reentry back to earth, blood samples showed a 17% loss of blood plasma, which contributed to a decline of erythropoietin secretion.[[48]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-48)[[49]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-49) On the skeletal system which is important to support our body's posture, long space flight and exposure to microgravity cause demineralization and atrophy of muscles. During re-acclimation, astronauts were observed to have a myriad of symptoms including cold sweats, nausea, vomiting and motion sickness.[[50]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-50) Returning astronauts also felt disoriented. Journeys to and from Mars being six months is the average time spent at the ISS. Once on Mars with its lesser surface gravity (38% percent of Earth's), these health effects would be a serious concern.[[51]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-51) Upon return to Earth, recovery from bone loss and atrophy is a long process and the effects of microgravity may never fully reverse.[[*citation needed*](https://en.wikipedia.org/wiki/Wikipedia:Citation_needed)]

#### Radiation**[**[**edit**](https://en.wikipedia.org/w/index.php?title=Colonization_of_Mars&action=edit&section=14)**]**

Because of so much radiation reaching Mars' surface, the planet has lost its inner [dynamo](https://en.wikipedia.org/wiki/Dynamo_theory) despite its far distance from the Sun compared to Earth. Due to this, Mars has a weaker global [magnetosphere](https://en.wikipedia.org/wiki/Magnetosphere) than Earth does. Combined with a thin atmosphere, this permits a significant amount of [ionizing radiation](https://en.wikipedia.org/wiki/Ionizing_radiation) to reach the Martian surface. There are two main types of radiation risks to traveling outside the protection of Earth's atmosphere and magnetosphere: galactic cosmic rays (GCR) and solar energetic particles (SEP). Earth's magnetosphere protects from charged particles from the Sun, and the atmosphere protects against uncharged and highly energetic GCRs. There are ways to mitigate against solar radiation, but without much of an atmosphere, the only solution to the GCR flux is heavy shielding amounting to roughly 15 centimeters of steel, 1 meter of rock, or 3 meters of water, limiting human colonists to living underground most of the time.[[52]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-52)

*Further information:*[*Health threat from cosmic rays*](https://en.wikipedia.org/wiki/Health_threat_from_cosmic_rays)

The [Mars Odyssey](https://en.wikipedia.org/wiki/2001_Mars_Odyssey) spacecraft carries an instrument, the [Mars Radiation Environment Experiment](https://en.wikipedia.org/wiki/Mars_Radiation_Environment_Experiment) (MARIE), to measure the radiation. MARIE found that radiation levels in orbit above Mars are 2.5 times higher than at the [International Space Station](https://en.wikipedia.org/wiki/International_Space_Station). The average daily dose was about 220 μGy (22 mrad)—equivalent to 0.08 Gy per year.[[53]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-53) A three-year exposure to such levels would exceed the safety limits currently adopted by NASA,[[54]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-54) and the risk of developing cancer due to radiation exposure after a Mars mission could be two times greater than what scientists previously thought.[[55]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-55)[[56]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-56) Occasional [solar proton events](https://en.wikipedia.org/wiki/Solar_proton_event) (SPEs) produce much higher doses, as observed in September 2017, when NASA reported radiation levels on the surface of Mars were temporarily [doubled](https://en.wikipedia.org/wiki/Orders_of_magnitude_(radiation)), and were associated with an [aurora](https://en.wikipedia.org/wiki/Aurora) 25-times brighter than any observed earlier, due to a massive, and unexpected, [solar storm](https://en.wikipedia.org/wiki/Coronal_mass_ejection).[[57]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-PHYS-20170930-57) Building living quarters underground (possibly in [Martian lava tubes](https://en.wikipedia.org/wiki/Martian_lava_tube)) would significantly lower the colonists' exposure to radiation.

[](https://en.wikipedia.org/wiki/File:PIA17601-Comparisons-RadiationExposure-MarsTrip-20131209.png)

Comparison of radiation doses—includes the amount detected on the trip from Earth to Mars by the [RAD](https://en.wikipedia.org/wiki/Radiation_assessment_detector) on the [MSL](https://en.wikipedia.org/wiki/Mars_Science_Laboratory) (2011–2013).[[58]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-SCI-20130531a-58)[[59]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-SCI-20130531b-59)[[60]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-NYT-20130530-60)

Much remains to be learned about space radiation. In 2003, NASA's [Lyndon B. Johnson Space Center](https://en.wikipedia.org/wiki/Lyndon_B._Johnson_Space_Center) opened a facility, the [NASA Space Radiation Laboratory](https://en.wikipedia.org/wiki/NASA_Space_Radiation_Laboratory), at [Brookhaven National Laboratory](https://en.wikipedia.org/wiki/Brookhaven_National_Laboratory), that employs [particle accelerators](https://en.wikipedia.org/wiki/Particle_accelerator) to simulate space radiation. The facility studies its effects on living organisms, as well as experimenting with shielding techniques.[[61]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-61) Initially, there was some evidence that this kind of low level, chronic radiation is not quite as dangerous as once thought; and that [radiation hormesis](https://en.wikipedia.org/wiki/Radiation_hormesis) occurs.[[62]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-zubrin1996b-62) However, results from a 2006 study indicated that protons from cosmic radiation may cause twice as much serious damage to [DNA](https://en.wikipedia.org/wiki/DNA) as previously estimated, exposing astronauts to greater risk of cancer and other diseases.[[63]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-spaceRdiation-63) As a result of the higher radiation in the Martian environment, the summary report of the [Review of U.S. Human Space Flight Plans Committee](https://en.wikipedia.org/wiki/Review_of_U.S._Human_Space_Flight_Plans_Committee) released in 2009 reported that "Mars is not an easy place to visit with existing technology and without a substantial investment of resources."[[63]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-spaceRdiation-63) NASA is exploring a variety of alternative techniques and technologies such as [deflector shields](https://en.wikipedia.org/wiki/Deflector_shield) of plasma to protect astronauts and spacecraft from radiation.[[63]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-spaceRdiation-63)

#### Psychological effects**[**[**edit**](https://en.wikipedia.org/w/index.php?title=Colonization_of_Mars&action=edit&section=15)**]**

Due to the communication delays, new protocols need to be developed in order to assess crew members' psychological health. Researchers have developed a Martian simulation called [HI-SEAS](https://en.wikipedia.org/wiki/HI-SEAS) (Hawaii Space Exploration Analog and Simulation) that places scientists in a simulated Martian laboratory to study the psychological effects of isolation, repetitive tasks, and living in close-quarters with other scientists for up to a year at a time. Computer programs are being developed to assist crews with personal and interpersonal issues in absence of direct communication with professionals on Earth.[[64]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-64) Current suggestions for Mars exploration and colonization are to select individuals who have passed [psychological screenings](https://en.wikipedia.org/wiki/Psychiatric_assessment). Psychosocial sessions for the return home are also suggested in order to reorient people to society.

### Terraforming

### Minimum size of a colony**[**[**edit**](https://en.wikipedia.org/w/index.php?title=Colonization_of_Mars&action=edit&section=17)**]**

To be self-sustaining, a colony would have to be large enough to provide all the necessary living services. These include[[66]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-Salotti-66)

* **Ecosystem management**: producing appropriate gases, controlling air composition pressure and temperature, collecting and producing water, growing food and processing organic wastes.
* **Energy production**: this includes extracting methane for vehicles and if photovoltaic cells are used to produce energy this would include the extraction and processing of silicates, to augment or replace any original equipment.
* **Industry**: extracting and processing appropriate ores, manufacturing tools and other objects; producing clothes, medicine, glass, ceramics, plastics.
* **Building**: even if the base is constructed before arrival, it will need frequent adaptation according to the evolution of the settlement as well as inevitable replacement.
* **Social activities**: this includes raising children and educating them, health care, preparing meals, cleaning, washing, organizing the work and making decisions. Time for sport, culture and entertainment can be minimized but not eliminated.

As the number of individuals grows, both activities and objects can be shared between them. Growth also will offset the risks of collapse of the society, caused by sudden deaths, accidents, infertility or inbreeding. But this may not prevent mortal combat between different groups of individuals, or the loss of efficiency due to inappropriate social organization.

By mathematical modelling of the time spent by people on these issues and by keeping things simple, Salotti concludes that the minimum number for a colony on Mars is 110.[[66]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-Salotti-66) This is close to other studies of the genetic problems involved in the longer journey to [Proxima Centauri b](https://en.wikipedia.org/wiki/Proxima_Centauri_b" \o "Proxima Centauri b) (6,000+ years).[[67]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-67)

## Equipment needed for colonization[[edit](https://en.wikipedia.org/w/index.php?title=Colonization_of_Mars&action=edit&section=21)]

Colonization of Mars would require a wide variety of equipment—both equipment to directly provide services to humans and [production equipment](https://en.wikipedia.org/wiki/Capital_(economics)) used to produce food, propellant, water, energy and breathable oxygen—in order to support human colonization efforts. Required equipment will include:[[1]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-zubrin1996-1)

* Basic [utilities](https://en.wikipedia.org/wiki/Utilities) ([oxygen](https://en.wikipedia.org/wiki/Oxygen), [power](https://en.wikipedia.org/wiki/Electricity_generation), [local communications](https://en.wikipedia.org/wiki/Communications_system), [waste disposal](https://en.wikipedia.org/wiki/Waste_disposal), [sanitation](https://en.wikipedia.org/wiki/Sanitation) and [water recycling](https://en.wikipedia.org/wiki/Reclaimed_water#Reuse_in_space_stations))
* [Habitats](https://en.wikipedia.org/wiki/Mars_habitat)
* Storage facilities
* workspaces
* Airlock, for pressurization and dust management
* [Resource extraction equipment](https://en.wikipedia.org/wiki/In-situ_resource_utilization)—initially for [water](https://en.wikipedia.org/wiki/Chronology_of_discoveries_of_water_on_Mars) and oxygen, later for a wider cross section of minerals, building materials, etc.
* Equipment for [energy production](https://en.wikipedia.org/wiki/Energy_production) and [energy storage](https://en.wikipedia.org/wiki/Energy_storage), some [solar](https://en.wikipedia.org/wiki/Solar_panels_on_spacecraft) and perhaps [nuclear](https://en.wikipedia.org/wiki/Nuclear_power_in_space) as well

[](https://en.wikipedia.org/wiki/File:Mars_Greenhouse.jpg)

Mars greenhouses feature in many colonization designs, especially for food production and other purposes

[](https://en.wikipedia.org/wiki/File:Possible_exploration_of_the_surface_of_Mars.jpg)

Various technologies and devices for Mars are shown in the illustration of a Mars base

* [Food](https://en.wikipedia.org/wiki/Plants_in_space) [production](https://en.wikipedia.org/wiki/Space_farming) spaces and equipment.
* [Propellant production equipment](https://en.wikipedia.org/wiki/In-situ_resource_utilization#Rocket_propellant), generally thought to be [hydrogen](https://en.wikipedia.org/wiki/Hydrogen_rocket_fuel) and [methane](https://en.wikipedia.org/wiki/Liquid_methane) through the [Sabatier reaction](https://en.wikipedia.org/wiki/Sabatier_reaction)[[78]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-nsf20140307-78) for fuel—with [oxygen](https://en.wikipedia.org/wiki/Liquid_oxygen) oxidizer—for chemical rocket engines
* Fuels or other energy source for use with surface transportation. [Carbon monoxide](https://en.wikipedia.org/wiki/Carbon_monoxide)/[oxygen](https://en.wikipedia.org/wiki/Oxygen) (CO/O2) engines have been suggested for early surface transportation use as both carbon monoxide and oxygen can be straightforwardly produced by [zirconium dioxide](https://en.wikipedia.org/wiki/Zirconium_dioxide) [electrolysis](https://en.wikipedia.org/wiki/Electrolysis) from the [Martian atmosphere](https://en.wikipedia.org/wiki/Martian_atmosphere) without requiring use of any of the Martian water resources to obtain hydrogen.[[79]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-landis2001-79)
* Off-planet communication equipment
* Equipment for moving over the surface—[Mars suit](https://en.wikipedia.org/wiki/Mars_suit), [crewed rovers](https://en.wikipedia.org/wiki/Crewed_Mars_rover) and possibly even [Mars aircraft](https://en.wikipedia.org/wiki/Mars_aircraft).

### Basic utilities**[**[**edit**](https://en.wikipedia.org/w/index.php?title=Colonization_of_Mars&action=edit&section=22)**]**

In order to function at all the colony would need the basic utilities to support human civilization. These would need to be designed to handle the harsh Martian environment and would either have to be serviceable while wearing an EVA suit or housed inside a human habitable environment. For example, if electricity generation systems rely on solar power, large energy storage facilities will also be needed to cover the periods when dust storms block out the sun, and automatic dust removal systems may be needed to avoid human exposure to conditions on the surface.[[27]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-Fenton-27) If the colony is to scale beyond a few people, systems will also need to maximise use of local resources to reduce the need for resupply from Earth, for example by recycling water and oxygen and being adapted to be able to use any water found on Mars, whatever form it is in.

## Robotic precursors[[edit](https://en.wikipedia.org/w/index.php?title=Colonization_of_Mars&action=edit&section=24)]

[](https://en.wikipedia.org/wiki/File:Astronauts_approach_Viking_2.jpg)

Astronauts approach [*Viking 2*](https://en.wikipedia.org/wiki/Viking_2) lander probe

The path to a human colony could be prepared by [robotic](https://en.wikipedia.org/wiki/Robotic_spacecraft) systems such as the [Mars Exploration Rovers](https://en.wikipedia.org/wiki/Mars_Exploration_Rover) [*Spirit*](https://en.wikipedia.org/wiki/Spirit_rover), [*Opportunity*](https://en.wikipedia.org/wiki/Opportunity_rover), [*Curiosity*](https://en.wikipedia.org/wiki/Curiosity_rover) and [*Perseverance*](https://en.wikipedia.org/wiki/Perseverance_rover). These systems could help locate resources, such as ground water or ice, that would help a colony grow and thrive. The lifetimes of these systems would be years and even decades, and as recent developments in [commercial spaceflight](https://en.wikipedia.org/wiki/Commercial_spaceflight) have shown, it may be that these systems will involve private as well as government ownership. These robotic systems also have a reduced cost compared with early crewed operations, and have less political risk.

Wired systems might lay the groundwork for early crewed landings and bases, by producing various consumables including fuel, oxidizers, water, and construction materials. Establishing power, communications, shelter, heating, and manufacturing basics can begin with robotic systems, if only as a prelude to crewed operations.

[Mars Surveyor 2001 Lander](https://en.wikipedia.org/wiki/Mars_Surveyor_2001_Lander) MIP (Mars ISPP Precursor) was to demonstrate manufacture of oxygen from the [atmosphere of Mars](https://en.wikipedia.org/wiki/Atmosphere_of_Mars),[[84]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-84) and test solar cell technologies and methods of mitigating the effect of [Martian dust](https://en.wikipedia.org/wiki/Martian_dust) on the power systems.[[85]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-85)[[*needs update*](https://en.wikipedia.org/wiki/Wikipedia:Manual_of_Style/Dates_and_numbers#Chronological_items)]

Before any people are transported to Mars on the notional 2020s [Mars transportation infrastructure](https://en.wikipedia.org/wiki/SpaceX_Mars_transportation_infrastructure) envisioned by [SpaceX](https://en.wikipedia.org/wiki/SpaceX" \o "SpaceX), a number of robotic cargo missions would be undertaken first in order to transport the requisite [equipment](https://en.wikipedia.org/wiki/Mars_colonization_equipment), [habitats](https://en.wikipedia.org/wiki/Mars_habitat) and supplies.[[86]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-tss20140321gs-86) Equipment that would be necessary would include "machines to produce fertilizer, methane and oxygen from Mars' atmospheric nitrogen and carbon dioxide and the planet's subsurface water ice" as well as construction materials to build transparent domes for initial agricultural areas.[[87]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-dn20121213-87)

## Possible locations for settlements[[edit](https://en.wikipedia.org/w/index.php?title=Colonization_of_Mars&action=edit&section=27)]

[](https://en.wikipedia.org/wiki/File:Pavonis_Mons_lava_tube_skylight_crop.jpg)

Cropped version of a [HiRISE](https://en.wikipedia.org/wiki/HiRISE) image of a lava tube skylight entrance on the Martian volcano [Pavonis Mons](https://en.wikipedia.org/wiki/Pavonis_Mons" \o "Pavonis Mons).

### Equatorial regions**[**[**edit**](https://en.wikipedia.org/w/index.php?title=Colonization_of_Mars&action=edit&section=28)**]**

*See also:*[*Caves of Mars Project*](https://en.wikipedia.org/wiki/Caves_of_Mars_Project)

[Mars Odyssey](https://en.wikipedia.org/wiki/Mars_Odyssey) found what appear to be natural caves near the volcano [Arsia Mons](https://en.wikipedia.org/wiki/Arsia_Mons" \l "Possible_cave_entrances" \o "Arsia Mons). It has been speculated that settlers could benefit from the shelter that these or similar structures could provide from radiation and micrometeoroids. Geothermal energy is also suspected in the equatorial regions.[[96]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-96)

### Lava tubes**[**[**edit**](https://en.wikipedia.org/w/index.php?title=Colonization_of_Mars&action=edit&section=29)**]**

Several possible [Martian lava tube](https://en.wikipedia.org/wiki/Martian_lava_tube) skylights have been located on the flanks of Arsia Mons. Earth based examples indicate that some should have lengthy passages offering complete protection from radiation and be relatively easy to seal using on-site materials, especially in small subsections.[[97]](https://en.wikipedia.org/wiki/Colonization_of_Mars#cite_note-97)

### Hellas Planitia**[**[**edit**](https://en.wikipedia.org/w/index.php?title=Colonization_of_Mars&action=edit&section=30)**]**

[Hellas Planitia](https://en.wikipedia.org/wiki/Hellas_Planitia) is the lowest lying plain below the Martian [geodetic datum](https://en.wikipedia.org/wiki/Datum_(geodesy)). The air pressure is relatively higher in this place when compared to the rest of Mars.

# The Home on Mars

Home on Mars is a difficult concept to define. Even on Earth, the concept varies from person to person with different cultural background or from different geological location. Still the common component in everyone‟s very unique definition of home is

„comfort‟. As Juhani Pallasmaa states, *“The experience of home is essentially an experience of warmth. The space of warmth around the fire place is the space of ultimate intimacy and comfort. A sense of homecoming is never stronger than seeing a light in the window of a house in a snow-covered landscape at dusk; the remembrance of its warm interior gently warms one’s frozen limbs. Home and skin turn into a single sensation.”* [5] [Pallasmaa, An Architecture of Seven Senses] Here it would be important to point out the Pallasmaa is writing from a northern European conception of home that is closely tied to that culture and climate. The conception of home for an another climate and culture will be radically different, but in each case the imagery and physical sensations will support physical and psychological comfort. Basically, our concept of home mostly depends on this psychological comfort zone, which is a complex combination of memory and personal touch. As physician Jerri Nielsen described in her autobiography *“Home – what a concept. I was forty-six years old and living in my parents’ house, sleeping in a bedroom decorated with the ruffle curtains and daisy wallpaper of my teenage years.”* [6] [Nielsen with Vollers, Ice bound] So, on Earth we can recreate the appearance of home with specific decoration and rearranging our personal belongings according to our own choice to some extends, no matter we live in a foreign country or in a remote place like the research stations of Antarctica or of any desert. However, it is hard to recreate the „feelings of home‟. This special „feelings of home‟ represents one‟s very personal psychological state, which contents not only the physical existence of a house, but also all the surrounding environments where the house exists along with the complex web of passed time. Thus, every individual‟s concept of home has a singular physical and psychological existence that is intangible even here on Earth. Therefore, how will we perform this nearly

impossible job (creation of home) on an alien planet like Mars, where, even one small bedroom for each astronaut will be considered as an ultimate luxury? In addition, how is it possible to create a universal homelike environment, when each member of the small group of astronauts/scientists may have different taste, cultural background and therefore a different concept of home?

Fortunately, this selected group of people for the first manned mission to Mars will not be extreme level of home sick, as they will be tested and trained (both physically and psychologically) for several times beforehand. Still, we do not know how long they will be able to keep their controlled mental strength in any kind of unknown/unpredictable situation during their journey and stay on Mars. At least, we should ensure a psychologically healthy environment for the known/predictable difficult situations, so that they can perform with full mental strength at time of unknown emergency. To do so, first we need to identify the problems/difficulties they will face in normal situation and then go for the possible solutions. Here are some questions for which we are searching the suitable answers:

How we will solve the loneliness of those astronauts? How we can make sure that they will not be depressed or stressed at that hostile planet? How we can provide them the memory of earth‟s beautiful nature? The astronaut Scott Kelly said in one of his interview that he missed the fresh air mostly, in a way he cannot explain, while there was fresh air supply in International Space Station*.”* [7] [Kelly, Interview with CNN] Is it the memory of free flowing earth‟s fresh air? How we will recover the extreme silence of Mars? In our earth we have never experienced such silence. How will we ensure them the mental calmness when they will miss the chirping of birds, the sound of flowing water, the simple sound of dried leafs or even the familiar noises and patterns of urban life? Are those artificial recorded sounds of CD players will be enough for those situations?

Through an analytical and comparative study of the following case studies, I will try to demonstrate possible design solutions for these questions. I will look at both technical and non-technical aspects. Relative to Survivability, I will identify technical solutions to the habitat construction method, enclosure strategy and materials, defenses against radiation, pressure and gravity, action plans for food and water. Relative to Livability I

will assess non-technical solutions to problems of restricted access, limited space, communal and private spaces and connection to one‟s personal sense of home.

# Case Study 1: “The Ice House”

Project type: First prize winner of the 3-D Printed Habitat Challenge Design Competition by NASA.

Architect/team: Space Exploration Architecture and Clouds Architecture Location: Mars

The proposal uses a lander as the basis of the shelter, containing both private and communal interior spaces. Once in place, an inflatable membrane is used to create an interstitial environment between the outside of the capsule and the Mars atmosphere. Rovers would then extract water from the ice below the surface at Alba Mons and apply it to form a protective skin on the inside of the inflatable environment. This solution will also create a 'backyard' where astronauts can enter using just an oxygen mask.



(Fig:1) Mars Ice House is 3D printed from translucent ice, which shields the crew from radiation and transforms into a glowing beacon in the Martian night.




Fig: 2, The sectional perspective with plans of Martian Ice House, edited by me




Fig: 3, study sketch by author

The proposal looks very reasonable. However, it raises some questions at the same time: Is “Using the Ice of Mars” to build a house will be a great decision, while the limited iced water has other vital purpose to serve? From the rendering it seems a total contrast with the surrounding: Igloo in a red desert! This may be a good solution for radiation protection and day light. However, the refraction of this heavily layered ice wall will not allow the proper exterior view from inside. Mainly the inhabitants will live in some quarters in the core of the structure. What will be their psychological impact for living in such a small, closed and introvert space for long term basis?

# Case Study 2: “The Modular Habitat”

Project type: 2nd prize winner of the 3-D Printed Habitat Challenge Design Competition by NASA.

Architect/team: Team Gamma, architects Foster and Partners Location: Mars

The habitat will be delivered in two stages prior to the arrival of the astronauts. First, semi-autonomous robots select the site and dig a 1.5 meter deep crater. Then the larger 'Diggers' will create the crater by excavating the regolith, which the medium- sized 'Transporters' then move into position over the inflatable habitat modules layer by layer. The loose Martian soil is then fused using microwaves around the modules using the same principles involved in 3D-printing by several small 'Melters'. The fused regolith creates a permanent shield that protects the settlement from excessive radiation and extreme outside temperatures.

In their design Foster and Partners have proposed a solution that is related to our memory of Earth habitation – court yard and the shape of hut. This design is considering the Mars‟s undulating topography and also the main construction material is primarily very available „the Mars Soil‟ (fig: 5)

Step 1 Step 2





Step 3 Final product

Fig: 4, The Modular Habitat construction steps.



Fig: 5, study sketches by author



Fig: 6, The design of the compact 93 sqm habitat modules combines spatial efficiency with human physiology and psychology, with overlapping private and communal spaces.

In comparison to the Ice house I think this proposal is more sensitive in terms of using materials and merge the habitat with its original natural contest. However, the contraction process is too much dependent on robots, which has to be built first. In addition, the interior rendering is too close science fiction movie set. Is there any necessity to create a „science fiction type‟ living space just because the location is Mars?

Though there are provisions for false windows, they are not operable at all, neither functionally nor visually. Windows have great positive impact on human psychology for a small confined space, which is the reason we use the windows in air planes, though it increases the cost of construction. On Mars, to provide the transparency of windows may be more difficult in terms of both safety and cost, however, we can use the digital projection of natural scenes on fake windows to create an illusion of Earth‟s soothing nature.

# Case Study 3: “The International Space Station”

Location: Near orbital of earth

